DTC A1-1x (A1-10 to A1-19, A1-1A to A1-1F): Faulty Power Supply (VA line) Check the No. 10 (7.5 A) fuse in the under-dash fuse/relay box. Is the fuse OK?
YES | - | Go to Step 2 .
NO | - | Short to ground in the under-dash fuse/relay box No.10 (7.5 A) fuse circuit.■
Turn the ignition switch ON (II) and wait for 30 seconds. Then turn the ignition switch OFF. Disconnect SRS unit connector A (28P) from the SRS unit. Reconnect the battery negative cable. |