1. Tighten the bolts in sequence to the specified torque.
   Specified Torque
   8 mm Bolts: | 22 N·m (22 kgf·m, 16 lbf·ft)
   6 mm Bolts: | 12 N·m (1.2 kgf·m, 8.7 lbf·ft)
   6 mm Bolts: | (21), (22), (23)
Install the cam chain. Install the engine wire harness connectors and wire harness clamps to the cylinder head. Four injector connectors Four glow plug connectors Engine coolant temperature (ECT) sensor connector Camshaft position (CMP) sensor connector Turbocharger boost control solenoid connector Install the fuel pump. Install the exhaust gas recirculation (EGR) valve. Install the exhaust manifold. Install the intake manifold. |