1. Apply a light coat of primer, then apply a double-sided adhesive tape (A) to the molding (B) as shown. Attach the fastener (C) with adhesive tape to the inside face of the quarter glass (D): Be sure the fastener lines up with the alignment marks (E). Be careful not to touch the quarter glass where adhesive will be applied. Do not peel the separators off the double-sided adhesive tape.
   Double-sided adhesive tape:
   | Thickness 0.6 mm (0.02 in.)
   | Width 4 mm (0.16 in.)
   Fastener adhesive tape:
   | Thickness 0.6 mm (0.02 in.)
   | Width 7.5 mm (0.3 in.)