Install the opener cable in the reverse order of removal, and note these items: Align the marks (A) on the opener cable (B) with the cable clips (C) and cushion tape (D) as shown. RHD: Align the marks (A) on the opener cable (B) routed along the middle floor cross member with hole seals (E) (without side curtain airbag) or harness clips (F) (with side curtain airbag) as shown. Replace any damaged clips, and replace the cushion tape. | LHD RHD