A/T Housing Bearing Removal

Special Tools Required Driver attachment, 78 x 90 mm 07GAD-SD40101 Handle driver 07749-0010000 Driver attachment, 42 x 47 mm 07746-0010300 Snap ring pliers 07LGC-0010100 Remove the idler gear shaft when removing the mainshaft bearing and idler gear shaft bearing. NOTE: If you are only removing the countershaft bearing, idler gear shaft removal is not needed. To remove the mainshaft bearing (A) and countershaft bearing (B) from the transmission housing, expand each snap ring with the snap ring pliers, then push the bearing out. NOTE: Do not remove the snap ring unless it's necessary to clean the grooves in the housing. |

Expand the snap ring of the idler gear shaft bearing with the snap ring pliers, then push the bearing out. |