Starter (MITSUBISHI)

Item | Measurement | Qualification | Standard or New | Service Limit
--- | --- | --- | --- | ---
Starter (MITSUBISHI) | Output |  | 1.7 kW
Commutator mica depth |  | 0.4−0.6 mm (0.016−0.024 in.) | 0.2 mm (0.008 in.)
Commutator runout |  | 0.05 mm (0.002 in.) max. | 0.1 mm (0.004 in.)
Commutator O.D. |  | 29.3−29.5 mm (1.154−1.161 in.) | 28.8 mm (1.134 in.)
Brush length |  | 7.7−8.0 mm (0.30−0.31 in.) | 0.9 mm (0.04 in.)