1. Remove the camshaft holders. Measure the widest portion of plastigage on each journal. If the camshaft-to-holder clearance is within limits, go to Step 11 . If the camshaft-to-holder clearance is beyond the service limit and the camshaft has been replaced, replace the cylinder head. If the camshaft-to-holder clearance is beyond the service limit and the camshaft has not been replaced, go to Step 10 . Camshaft-to-Holder Oil Clearance
   Standard (New): |
   No. 1 Journal: | 0.030−0.069 mm (0.001−0.003 in.)
   No. 2, 3, 4, 5 Journals: | 0.060−0.099 mm (0.002−0.004 in.)
   Service Limit: | 0.15 mm (0.006 in.)