Pull back the edge of the seat-back cover (A) all the way around, and release the clips (B), then remove the seat-back cover. Install the cover in the reverse order of removal, and note these items: To prevent wrinkles, make sure the material is stretched evenly over the pad before securing the clips. Replace any clips you removed with new ones. Install them with commercially available upholstery ring pliers. | Left seat-back Right seat-back