Distance Switch Test

Remove the switch cover (A). Remove the distance switch (B), then disconnect the 8P connector (C). Check for continuity between the 8P connector No. 3 and No. 8 terminals. There should be continuity with the distance switch pressed. There should be no continuity with the distance switch released. If the continuity check is not as specified, replace the cruise control combination switch assembly. |