DTC Troubleshooting: 12

DTC 12: Torque Sensor PVF Turn the ignition switch ON (II). Clear the DTC with the HDS. Start the engine. Wait at least 10 seconds. Does the EPS indicator come on?
YES | - | Go to Step 5 .
NO | - | The system is OK at this time.■
Stop the engine, and verify the DTC. Is DTC 12 indicated?
YES | - | Check for loose terminals and poor connections at the EPS control unit. If necessary, substitute a known-good EPS control unit and recheck.■
NO | - | Perform the appropriate troubleshooting for the code indicated.■