DTC P1298: ELD Circuit High Voltage NOTE: Information marked with an asterisk ( * ) applies to the 2004 model. Information marked with double asterisk ( ** ) applies to the 2005 model. Turn the ignition switch ON (II). Check the ELECTRICAL LOAD DETECTOR in the DATA LIST with the HDS. Is 0.2 A or less indicated?
YES | - | Go to Step 3 .
NO | - | Intermittent failure, system is OK at this time. Check for poor connections or loose terminals at the ELD and the ECM.■
Turn the ignition switch OFF. Disconnect the ELD 3P connector. Turn the ignition switch ON (II). Measure voltage between ELD 3P connector terminal No. 1 and body ground. Is there battery voltage?
YES | - | Go to Step 7 .
NO | - | 2004 model: Repair open in the wire between No. 8 FI ECU (ECM) (20 A) fuse and the ELD, then go to Step 15 . 2005 model: Repair open in the wire between No. 18 IG ACG (15 A) fuse and the ELD, then go to Step 15 .
Turn the ignition switch OFF, and wait 30 seconds. Disconnect ECM connector No. 2 (58P). |