Check for continuity between shift solenoid harness connector terminal No. 3 and body ground. Is there 12−25 Ω?
YES | - | Repair open in the wire between PCM connector terminal C3 and the shift solenoid harness connector, then go to Step 13 .
NO | - | Check shift solenoid valve E, and check for an open in the shift solenoid harness in the transmission. Replace shift solenoid valve E and/or shift solenoid harness, then go to Step 13 .
Clear the DTC with the HDS. Start the engine, and shift the transmission in 2nd gear in the M position. Monitor the OBD status for P0986 in the DTCs/Freeze Data in A/T Mode Menu for a pass/fail. Does the result indicate a pass?
YES | - | The problem has been corrected.■
NO | - | Return to Step 1 and recheck.■