ECM/PCM Inputs and Outputs at Connector D (17P)
NOTE: Standard battery voltage is 12 V.

Terminal number | Wire color | Terminal name | Description | Signal
--- | --- | --- | --- | ---
2 *4 | BRN | SMODE (SEQUENTIAL SPORT SHIFT MODE) | Detects sequential sportshift mode switch signal | In sequential sportshift mode (shift lever is positioned in sequential sportshift mode): 0 V In other than sequential sportshift mode: about 5 V
3 *4 | WHT | SUP (UPSHIFT SWITCH) | Detects upshift switch signal | In sequential sportshift mode and shift lever pushed toward upshift position: 0 V In sequential sportshift mode and shift lever in neutral position: about 5 V
5 *4 | GRN | ATPR (TRANSMISSION RANGE SWITCH R POSITION) | Detects transmission range switch R position signal | In R position: about 0 V In any other position: battery voltage
6 *4 | BLU | ATPP (TRANCMISSION RANGE SWITCH PARK POSITION) | Detects transmission range switch Park position signal | In Park position: about 0 V In any other position: battery voltage
8 *2 | BRN | BKSWNC (BRAKE PEDAL POSITION SWITCH) | Detects brake pedal position switch signal | With ignition switch ON (II) and brake pedal released: battery voltage With ignition switch ON (II) and brake pedal pressed: about 0 V
9 *4 | ORN | SDN (DOWNSHIFT SWITCH) | Detects downshift switch signal | In sequential sportshift mode and shift lever pushed toward downshift position: 0 V In sequential sportshift mode and shift lever in neutral position: about 5 V
9 *5 | LT BLU | CRMTCLS (CRUISE CLUTCH PEDAL POSITION SIGNAL) | Detects cruise clutch pedal position switch signal | With ignition switch ON (II) and clutch pedal released: about 0 V With ignition switch ON (II) and clutch pedal pressed: battery voltage
10 *4 | LT GRN | METINH (METER DISPLAY INHIBIT SIGNAL) | Sends inhibit signal | With ignition switch ON (II): battery voltage
11 *3 | PNK | ATCCFWD (TRANSMISSION RANGE SWITCH CRUISE CONTROL FWD SIGNAL) | Sends Park and D3 transmission range switch signal to cruise control unit | In D, D3 position: about 0 V In any other than D, D3 position: battery voltage
12 *3 | ORN(BLU) *6 | CCS (CRUISE CONTROL SIGNAL) | Detects cruise control signal | With cruise control: pulses
15 *2 | BRN | DBWRLY (THROTTLE ACTUATOR CONTROL MODULE RELAY) | Drives throttle actuator control module relay | With ignition switch ON (II): 0 V

*2: | K24A3 engine
*3: | K20A6 engine
*4: | A/T
*5: | K24A3 engine (M/T)
*6: | RHD model