Fuel Gauge Sending Unit Replacement

Remove the fuel fill cap. Fold the rear seat and rise the seat cushion. Remove the access panel (A) from the floor. Disconnect the fuel pump 5P connector (B). Disconnect the quick-connect fitting (C) and hose (D) from the fuel tank unit. |

Remove the fuel tank unit (A). When connecting the fuel tank unit, make sure the connection is secure and the suction filter is firmly connected to the pipe. Install the part in the reverse order of removal with a new base gasket (B), and bleed the fuel system. |