Install the seat belt in the reverse order of removal, and note these items: Apply liquid thread lock to the upper anchor bolt before reinstallation. Check that the retractor locking mechanism functions. Assemble the washers, collars, and bushings on the upper and lower anchor bolts as shown. Before installing the anchor bolts, make sure there are no twists or kinks in the front seat belt. Make sure the seat belt tensioner connector is plugged in properly. Reconnect the negative cable to the battery. Reset the clock. Perform the power window control unit reset procedure. | Upper anchor bolt construction Lower anchor bolt construction