Special Tools Required Ball joint remover, 28 mm 07MAC-SL00201 or 07MAC-SL00200 Note these items during removal: Using solvent and a brush, wash any oil and dirt off the valve body unit, its lines, and the end of the gearbox. Blow dry with compressed air. Make sure to remove the steering wheel before disconnecting the steering joint. Damage to the cable reel can occur. The illustrations show LHD model, RHD model is symmetrical. Drain the power steering fluid. Raise the front of vehicle, and support it with safety stands in the proper locations. Remove the front wheels. Remove the steering wheel. Remove the steering joint cover A. |