Connecting rod

Item | Measurement | Qualification | Standard or New | Service Limit
--- | --- | --- | --- | ---
Connecting rod | Pin-to-rod clearance |  | 0.005−0.015 mm (0.0002−0.0006 in.) | 0.02 mm (0.0008 in.)
Small-end bore diameter |  | 21.970−21.976 mm (0.8650−0.8652 in.) | ———
Large-end bore diameter | K20Z2 engine | 48.0 mm (1.89 in.) | ———
K24A3 engine | 51.0 mm (2.01 in.) | ———
End play installed on crankshaft |  | 0.15−0.35 mm (0.006−0.014 in.) | 0.40 mm (0.016 in.)