Exhaust Camshaft Gear B Replacement

Remove the cylinder head cover. Hold the exhaust camshaft with an open-end wrench, then loosen the exhaust gear B mounting bolt. Remove the camshafts. |

1. Remove the exhaust camshaft gear B. Install the exhaust camshaft gear B. Install the camshafts. Apply new engine oil to the threads and flange of the exhaust camshaft gear B mounting bolt, and install it. Hold the exhaust camshaft with an open-end wrench, then tighten the bolt.
   Specified Torque: | 78 N·m (8.0 kgf·m, 58 lbf·ft)
Install the cylinder head cover. |