1. Marking the target position of the passenger's side Measuring distance YY mm from the mark (N) described in Step 16 to the passenger's side, and it put the mark (P) on the floor.
   Prescribed distance | Offset distance YY
   1,500 mm (59.055 in.) | 436 mm (17.165 in.)
   2,000 mm (78.74 in.) | 524 mm (20.629 in.)
   2,500 mm (98.425 in.) | 612 mm (24.094 in.)
   3,000 mm (118.11 in.) | 700 mm (27.559 in.)
NOTE: The distance YY depends on the prescribed distance X which is chosen in Step 3 . Choose the offset distance XX which corresponds to the chosen prescribed distance. |