Put the cartridge in a caulking gun, and run a bead of adhesive (A) around the edge of the quarter glass (B) as shown: After applying the adhesive, peel the separator off the butyl tape. Apply the adhesive within 30 minutes after applying the glass primer. Make slightly thicker bead at each corner. Fold the edge of the adhesive backing from the double-sided adhesive tape stuck in Step 9 . If old quarter glass is to be reinstalled, peel the adhesive backings from the butyl tapes. |