Recirculation Control Motor Replacement

NOTE: LHD type is shown, RHD type is symmetrical. Open the glove box. Remove the damper from the glove box hang down. Remove the relays from the bracket. |

Disconnect the 7P connector (A) from the recirculation control motor (B). Remove the self-tapping screws and the recirculation control motor from the blower unit. Install the motor in the reverse order of removal. Make sure the pin on the motor is properly engaged with the linkage. After installation, make sure the motor runs smoothly. |