1. SRS components are located in this area. Review the SRS component locations LHD, SRS component locations RHD and the precautions and procedures before performing repairs or service. NOTE: When prying components, use the handy remover set or equivalent. Have an assistant help you when removing and installing the dashboard. Take care not to scratch the dashboard, body and other related parts. Put on gloves to protect your hands. Disconnect the negative cable from the battery, and wait at least 3 minutes before beginning work. Remove these items: Center console Driver's dashboard lower cover Center pocket Glove box Kick panels, both sides Front pillar trim, both sides
   - | Without side curtain airbag
   - | With side curtain airbag
Steering column Shift lever, A/T model Shift lever housing, M/T model Stereo amplifier Remove the screw (A) and release the clip (B), then remove the driver's center lower cover (C). LHD is shown; RHD is symmetrical. |