DTC P0193: FRP Sensor Circuit High Voltage Turn the ignition switch ON (II). Check the FRP SENSOR in the DATA LIST with the HDS. Is about 4.75 V or higher indicated?
YES | - | Go to Step 3 .
NO | - | Intermittent failure, system is OK at this time. Check for poor connections or loose terminals at the FRP sensor and the ECM.■
Turn the ignition switch OFF, and wait 30 seconds. Disconnect the FRP sensor 3P connector. Connect FRP sensor 3P connector terminals No. 2 and No. 3 with a jumper wire. Turn the ignition switch ON (II). Check the FRP SENSOR in the DATA LIST with the HDS. Is about 4.75 V or higher indicated?
YES | - | Go to Step 8 .
NO | - | Go to Step 18 .
Remove the jumper wire from the FRP sensor 3P connector. |