DTC Troubleshooting: P0097 (10-5)

DTC P0097: IAT Sensor 2 Low Voltage Turn the ignition switch ON (II). Check IAT SENSOR 2 in the DATA LIST with the HDS. Is about 0.097 V or less indicated?
YES | - | Go to Step 3 .
NO | - | Intermittent failure, system is OK at this time. Check for poor connections or loose terminals at the MAP/IAT sensor and the ECM.■
Turn the ignition switch OFF. Disconnect the MAP/IAT sensor 4P connector. Turn the ignition switch ON (II). Check IAT SENSOR 2 in the DATA LIST with the HDS. Is about 0.097 V or less indicated?
YES | - | Go to Step 7 .
NO | - | Go to Step 10 .
Turn the ignition switch OFF, and wait 30 seconds. Disconnect ECM connector No. 1 (96P). Check for continuity between MAP/IAT sensor 4P connector terminal No. 3 and body ground. Is there continuity?
YES | - | Repair short in the wire between the MAP/IAT sensor and ECM connector No. 1 terminal No. 17, then go to Step 12 .
NO | - | Go to Step 16 .
Turn the ignition switch OFF. Replace the MAP/IAT sensor. Reconnect all connectors. Turn the ignition switch ON (II). Reset the ECM with the HDS. Check for Temporary DTCs or DTCs with the HDS. Are any Temporary DTCs or DTCs indicated?
YES | - | If DTC P0097 is indicated, check for poor connections or loose terminals at the MAP/IAT sensor and the ECM, then go to Step 1 . If any other Temporary DTCs or DTCs are indicated, go to the indicated DTC's troubleshooting.
NO | - | Troubleshooting is complete.■
Update the ECM if it does not have the latest software, or substitute a known-good ECM. Check for Temporary DTCs or DTCs with the HDS. Are any Temporary DTCs or DTCs indicated?
YES | - | If DTC P0097 is indicated, check for poor connections or loose terminals at the MAP/IAT sensor and the ECM, then go to Step 1 . If any other Temporary DTCs or DTCs are indicated, go to the indicated DTC's troubleshooting.
NO | - | If the ECM was updated, troubleshooting is complete. If the ECM was substituted, replace the original ECM. ■