Transmission Range Switch Test

Remove the transmission range switch harness connector (A) from the connector bracket (B), then disconnect the connector. |

Check for continuity between terminals at the harness connector. There should be continuity between the terminals in the following table for each switch position. | Transmission Range Switch Harness Connector 2003-2004 Models Transmission Range Switch Harness Connector 2005 Model

If there is no continuity between any terminals, remove the transmission range switch cover, and disconnect the connector at the switch. |

Check for continuity between terminals at the switch connector. There should be continuity between the terminals in the following table for each switch position. If the transmission range switch continuity check is OK, replace the faulty transmission range switch harness. | Transmission Range Switch Connector

1. If there is no continuity between any terminals, remove the transmission range switch, and check the end of the selector control shaft (A).
   Standard
   Selector Control Shaft Width (B):
   6.1−6.2 mm (0.240−0.244 in.)
   Selector Control Shaft End Gap (C):
   1.8−2.0 mm (0.07−0.08 in.)
The measurement of the control shaft end is within the standard, replace the transmission range switch. If the measurement is out of the standard, repair the selector control shaft end, and recheck the transmission range switch continuity. |