NOTE: Do not hold the shift solenoid connector to remove and to install the shift solenoid valves. Hold the shift solenoid valve body. Do not install the shift solenoid valve A before installing the shift solenoid valve D, and do not install shift solenoid valve B before solenoid valve E. If solenoid valves A and B are installed before solenoid valves D and E, it may damage the hydraulic control system. Remove the shift solenoid valves by holding the solenoid valve body. Install new O-rings (F) on each shift solenoid valves. NOTE: The new shift solenoid valve is equipped with new O-rings. If you install a new shift solenoid valve, there is no need to replace its O-rings. Install shift solenoid valve D by holding the shift solenoid valve body; be sure to install mounting bracket contacts the servo body. Install shift solenoid valve A by holding the shift solenoid valve body; be sure to install mounting bracket contacts the bracket on shift solenoid valve D. Install shift solenoid valve E by holding the shift solenoid valve body; be sure to install mounting bracket contacts the servo body. Install shift solenoid valve B by holding the shift solenoid valve body; be sure to install mounting bracket contacts the bracket on shift solenoid valve E. Install shift solenoid valve C by holding the shift solenoid valve body; be sure to install mounting bracket contacts the servo body. |