NOTE: Keep all foreign particles out of the transmission. Warm up the engine to normal operating temperature (the radiator fan comes on). Park the vehicle on level ground, and turn the engine off. NOTE: Check the fluid level within 60−90 seconds after turning the engine off. Remove the dipstick (yellow loop) (A) from the ATF dipstick guide pipe, and wipe it with a clean cloth. Insert the dipstick aligning the cap (B) with the guide tab (C). |