1. Tighten the rack guide screw (A) to 25 N·m (2.5 kgf·m, 18 lbf·ft), then loosen it. Retighten the rack guide screw to 3.9 N·m (0.4 kgf·m, 4 lbf·ft), then back it off to the specified angle.
   Specified return angle: | 15 °±5 °
Hold the rack guide screw stationary with a wrench, and tighten the locknut by hand until it's fully seated. Install the special tool on the locknut (B), and hold the rack guide screw stationary with a wrench. Tighten the locknut an additional 30 ° with the special tool. Check for unusual steering effort through the complete turning range. Check the steering wheel rotation play and the power assist. |