A/T Differential Carrier Bearing Replacement

Special Tools Required Attachment, 40 x 50 mm 07LAD-PW50601 NOTE: The bearing and bearing outer race should be replaced as a set. Inspect and adjust the carrier bearing preload whenever bearing is replaced. Check the bearing for wear and rough rotation. If the bearing is OK, removal is not necessary. Remove the carrier bearing (A) with a commercially available puller (B), bearing separator (C), and stepped adapter (D). |

Install the new bearings with the special tool using the small end and a press until it bottoms. Press the bearing on securely so there is no clearance between the bearing and the differential carrier. |