Install the stabilizer link (A) on the stabilizer bar (B) and the trailing arm (C) with the joint pins set at the center of their range of the movement. NOTE: The paint mark (D) on the stabilizer link shows the down direction. Install the new self-locking nut and flange nut, and lightly tighten them. NOTE: Use a new self-locking nut on reassembly. Place a jack under the knuckle, and raise the suspension to load it with the vehicle's weight. |