1. Install the trim in the reverse order of removal, and note these items: Replace the clips with new ones if it is damaged. Do not reuse the front pillar cap; always replace it. If the side curtain airbag has deployed, replace the front pillar trim with a new one. To prevent the side curtain airbags from deploying improperly and possibly causing injury, inspect removed pieces and replace them if they have any of these types of damage:
   - | Any cracks, deformations, or stress-whitenings in the front pillar trim (A)
   - | Any cracks, or stress-whitenings in the grommet and clip seating surfaces (B)
   - | Bent or broken grommet (C)
Replace any damaged parts with new ones. Make sure the top of the trim overlaps with the headliner correctly. Push the clips into place securely. |