Special Tools Required Driver attachment, 42 mm 07QAD-P0A0100 K20Z2 Engine Model Install the thrust needle bearing (A), needle bearing (B), 1st gear (C), thrust needle bearing (D), 40 x 51.5 mm thrust washer (E), 1st/3rd clutch (F), and 3rd gear collar (G) on the secondary shaft (H). Do not install the O-rings during inspection. Install the idler gear (I), then install the ball bearing (J) on the idler gear with the 42 mm driver attachment, and a press. Install the conical spring washer (K) and locknut (L), then tighten the locknut to 29 N·m (3.0 kgf·m, 22 lbf·ft). |