1. Install the headliner in the reverse order of removal, and note these items: If the side curtain airbag has been deployed, replace the headliner and front grab handle on deployed side with new ones. To prevent the side curtain airbags from deploying improperly and possibly causing injury, inspect removed pieces and replace them if they have any of these types of damage:
   - | Any creases or tears in the headliner (A)
   - | Any fasteners (B) or clip bases (C) which have come off the headliner
   - | Any damage around the grab handle holes (D) or sunvisor holes (E) in the headliner
   - | Any deformations in the grab handle (F)
   - | Any cracks in the sunvisor stay base (G)
   - | Any bends or cracks in the sunvisor stay shaft (H)
   - | Any cracks in the sunvisor base (I)
   - | Any cracks in the vanity mirror base (J)
   - | Any deformations in the grab handle bracket
Replace any damaged parts with new ones. Make sure the top of the headliner overlaps with the trim pieces correctly. When passing the headliner through the door opening, be careful not to fold or bend it. Also, be careful not to scratch the body. If the threads on a visor or grab handle screw is worn out, use an oversized self-tapping ET screw made specifically for this application: Visor: P/N 90137-S30-003 Grab handle: P/N 90137-S0A-003 Check that both sides of the headliner are securely attached to the trim. | Headliner Grab handle Sunvisor