F-CAN System Link F-CAN (Fast Controller Area Network) passes information between processors on the network. For example, the F-CAN network is used to pass fuel pulses between the PCM and the navigation unit for the trip computer function. The F-CAN network uses a communication protocol that transmits data at 500 Kbps. If the diagnostic screen below reads NG with the ignition switch ON (II), then diagnostic trouble codes (DTCs) for the F-CAN can be retrieved with the HDS (Honda Diagnostic System). The data displayed in the ID boxes is irrelevant. For more details on troubleshooting the F-CAN, refer to the multiplex system. |