M/T Clutch Housing Countershaft Bearing Replacement

Special Tools Required Oil seal driver 07JAD-PL90100 Adjustable bearing puller, 20−40 mm 07JAC-PH80100 Bearing remover shaft 07JAC-PH80200 Slide hammer 07741-0010201 Remove the bearing set plate (A) from the clutch housing (B). |

Remove the needle bearing (A) using the special tools, then remove the oil guide plate C. |

Position the oil guide plate C and new needle bearing (A) in the bore of the clutch housing (B). Install the needle bearing using the special tools. |

Install the bearing set plate (A) with bolts (B). |