NOTE: Take care not to scratch the door. Use a clip remover to remove the clips. At the center pillar, remove the door checker mounting bolt (A). Detach the clips (B, C, D), then remove the door weatherstrip (E). Install the weatherstrip in the reverse order of removal, and note these items: Replace any damaged clips. Make sure the weatherstrip is installed in the holder (F) securely. Apply liquid thread lock to the door checker mounting bolt before installation. Check for water leaks. |