Set the cable on the bracket (A).Turn the adjusting nut (B) so that its free play is 0 mm. Position the adjusting nut on the other side of the bracket, then tighten the locknut (C). With the cable properly adjusted, check the throttle link to be sure it opens fully when you push the accelerator pedal to the floor. Also check the throttle link to be sure it returns whenever you release the accelerator pedal. |