Monitor Check Overview of display unit The display unit communicates with the navigation unit over its own GA-Net bus. Information is sent to the navigation unit whenever the user activates the touch screen, or buttons. Information sent by the navigation unit to the display unit includes commands to control the LCD back light. The navigation unit also sends navigation and rear camera video information to the screen using the Red, Green, Blue, and Composite Video signals. The display unit is protected by the security system by daisy-chaining the security signal through it, and then passing the signal to the audio unit. The illumination input from the gauge brightness control provides back lighting for the buttons surrounding the screen. These screens allow troubleshooting of the display unit. Select the item you want to troubleshoot, and follow the diagnostic instructions. |