1. Disconnect the A/T clutch pressure control solenoid valves B and C connectors. Measure A/T clutch pressure control solenoid valve B resistance between the solenoid valve B terminals No. 1 and No. 2, and measure A/T clutch pressure control solenoid valve C resistance between the solenoid valve C terminals No. 1 and No. 2.
   Standard: | 3−10 Ω
If the resistance of either A/T clutch pressure control solenoid valve is out of standard, replace the A/T clutch pressure control solenoid valves B and C. Connect the battery positive terminal to the No. 1 terminal of the A/T clutch pressure control solenoid valves B and C connectors, and connect the battery negative terminal to the No. 2 terminal. A clicking sound should be heard. If no sound is heard, remove the A/T clutch pressure control solenoid valves B and C. Check the fluid passage of the A/T clutch pressure control solenoid valve for dust or dirt. |