Retainer Replacement Gradually scrape off the adhesive tape (A) under the retainers (B) while heating it with a heat gun. NOTE: Avoid overheating the painted surfaces around the retainers. Wrap the exterior resin parts near the front pillar with aluminum foil to protect them from overheating. Clean the body bonding surface with a sponge dampened in alcohol. After cleaning, keep oil, grease, and water from getting on the surface. |