1. Inspection (KQ Model) Raise the rear of the vehicle, and support it with safety stands in the proper locations. Remove the rear wheels. Check the thickness of the inner pad (A) and outer pad (B). Do not include the thickness of the brake pad backing plate.
   Brake pad thickness:
   | Standard: | 8.9−9.1 mm (0.350−0.358 in.)
   | Service limit: | 1.6 mm (0.06 in.)
If the brake pad thickness is less than the service limit, replace all the pads as a set. |