Special Tools Required Sub hanger stay 07MAK-PY30100 Engine tilt hanger set 07KAK-SJ40101 Engine hanger stay 07KAK-SJ40200 NOTE: Use fender covers to avoid damaging painted surfaces. To avoid damage, unplug the wiring connectors carefully while holding the connector portion. Mark all wiring and hoses to avoid misconnection. Also, be sure that they do not contact other wiring or hoses, or interfere with other parts. Make sure you have the anti-theft codes for the radio and navigation system, then write down the customer's audio presets. Make sure the ignition switch is OFF. Secure the hood in the wide open position (support rod in the lower hole). Relieve the fuel pressure. Disconnect the negative cable from the battery first, then the positive cable. Remove the battery. Disconnect the intake air temperature (IAT) sensor connector (A). Remove the vacuum hose (B) and breather pipe (C), then remove the intake air duct (D). |