DTC 32-3x (32-30 to 32-39, 32-3A to 32-3F): Short to Another Wire or Decreased Resistance in Right Side Airbag Inflator Special Tools Required SRS inflator simulator 07SAZ-TB4011A SRS simulator lead E 07XAZ-S1A0200 SRS short canceller 070AZ-SAA0100 Erase the DTC memory. Turn the ignition switch ON (II), and check that the SRS indicator comes on for about 6 seconds and then goes off. Does the SRS indicator stay on and is DTC 32-3x indicated?
YES | - | Go to Step 3 .
NO | - | Intermittent failure, system is OK at this time. Go to Troubleshooting Intermittent Failures. If another DTC is indicated, go to the DTC troubleshooting index for troubleshooting details.
Turn the ignition switch OFF. Disconnect the battery negative cable, and wait for 3 minutes. Disconnect the floor wire harness 2P connector (A) from the right side airbag. Connect the SRS inflator simulator (2 Ω connector) and simulator lead E to the floor wire harness. Reconnect the battery negative cable. Erase the DTC memory. Read the DTC. Is DTC 32-3x indicated?
YES | - | Go to Step 9 .
NO | - | Short to another wire in the right side airbag inflator; replace the right side airbag. ■
Turn the ignition switch OFF. Disconnect the battery negative cable, and wait for 3 minutes. |