1. Rear Toe Inspection/Adjustment Release the parking brake. Check the toe. If it is not within the specification, go to Step 3 .
   Rear toe-in: | 2±2 mm (0.08±0.08 in.)
Loosen the self-locking nut (A) while holding the adjusting bolt (B). Replace the self-locking nut with a new one, and lightly tighten it. NOTE: Always use a new self-locking nut whenever it has been loosened. Turn the adjusting bolt until the toe is correct. Tighten the self-locking nut to the specified torque while holding the adjusting bolt. |