Engine idle

Item | Measurement | Qualification | Standard or New
--- | --- | --- | ---
Engine idle | Idle speed without load | K20Z2 M/T (in neutral) | 650±50 rpm (min −1 )
K20Z2 A/T (in N or P position) | 650±50 rpm (min −1 )
K24A3 M/T (in neutral) | 650±50 rpm (min −1 )
K24A3 A/T (in N or P position) | 650±50 rpm (min −1 )
Idle speed with high electrical load (A/C switch ON, temperature set to max cool, blower fan on High, rear window defogger ON, and headlights on high beam) | K20Z2 M/T (in neutral) | 720±50 rpm (min −1 )
K20Z2 A/T (in N or P position) | 800±50 rpm (min −1 )
K24A3 M/T (in neutral) | 720±50 rpm (min −1 )
K24A3 A/T (in N or P position) | 800±50 rpm (min −1 )
Idle CO |  | 0.1 % max.