Cylinder Head Rocker Arm and Shaft Disassembly/Reassembly

NOTE: Identify parts as they are removed to ensure reinstallation in original location. Inspect the rocker arm shaft and rocker arms. The rocker arms must be installed in the same positions if reused. When removing or installing the rocker arm assembly, do not remove the camshaft holder bolts. The bolts will keep the holders and rocker arms on the shaft. Prior to reassembling, clean all the parts in solvent, dry them, and apply lubricant to any contact points. Bundle the intake rocker arms with rubber bands to keep them together as a set. When replacing the intake rocker arm assembly, remove the fastening hardwares from the new intake rocker arm assembly. | K20Z2 engine K24A3 engine