Intermediate Shaft Disassembly

Special Tools Required Oil seal driver 07947-SB00100 Half shaft base 07NAF-SR30101 Remove the set ring (A), outer seal (B), and external snap ring (C). |

Press the intermediate shaft (A) out of the intermediate shaft bearing (B) using a press. Be careful not to damage the metal rings (C) on the intermediate shaft during disassembly. |

Remove the internal snap ring. |

Press the intermediate shaft bearing (A) out of the bearing support (B) using the special tools and a press. |