DTC P0403: EGR Control Solenoid Valve Circuit Open Turn the ignition switch ON (II). Clear the DTC with the HDS. Start the engine. Hold the engine speed at 2,000 rpm (min −1 ) without load. Check for Temporary DTCs or DTCs with the HDS. Is DTC P0403 indicated?
YES | - | Go to Step 5 .
NO | - | Intermittent failure, system is OK at this time. Check for poor connections or loose terminals at the EGR control solenoid valve and the ECM.■
Check for Temporary DTCs or DTCs with the HDS. Are DTC P0045, P0403, and P2008 indicated at same time?
YES | - | Go to Step 6 .
NO | - | Go to Step 11 .
Turn the ignition switch OFF. Check the No. 10 IGP2 (20 A) fuse in the under-hood fuse/relay box. Is the fuse OK?
YES | - | Go to Step 8 .
NO | - | Repair short in the wire between the No. 10 IGP2 (20 A) fuse and PGM-FI main relay 2, then go to Step 22 . Repair short in the wire between PGM-FI main relay 2 and the EGR control solenoid valve, the EGR cooler bypass control solenoid valve, the IMRC solenoid valve, the reverse lock solenoid valve, the turbocharger boost control solenoid valve, the glow plug control module, the fuel heater relay, then go to Step 22 .
Disconnect PGM-FI main relay 2. Check PGM-FI main relay 2. Is PGM-FI main relay 2 OK?
YES | - | Go to Step 10 .
NO | - | Replace PGM-FI main relay 2, then go to Step 22 .
Measure voltage between PGM-FI main relay 2 4P connector terminal No. 1 and body ground. Is there battery voltage?
YES | - | Repair open in the wire between PGM-FI main relay 2 and the EGR control solenoid valve, the EGR cooler bypass control solenoid valve, the IMRC solenoid valve, the reverse lock solenoid valve, the turbocharger boost control solenoid valve, the glow plug control module, the fuel heater relay, then go to Step 22 .
NO | - | Repair open in the wire between the No. 10 IGP2 (20 A) fuse in the under-hood fuse/relay box and PGM-FI main relay 2, then go to Step 22 .
Turn the ignition switch OFF. Disconnect the EGR control solenoid valve 2P connector. Turn the ignition switch ON (II). |