Symptom: A/T gear position indicator does not indicate the shift lever position, the D indicator does not blink, and no transmission range switch DTCs are indicated. Turn the ignition switch ON (II). Measure the voltage between gauge assembly connector terminal B2 and body ground. The shift lever can be in any position. Is there battery voltage?
YES | - | Faulty A/T gear position indicator in the gauge assembly, replace the gauge assembly.■
NO | - | Go to Step 3 .