Connect the No. 2 terminal of the reverse lockout solenoid 2P connector to the battery positive terminal, and connect the No. 1 to the battery negative terminal. Check that the reverse lockout solenoid operates. Does the reverse lockout solenoid operate properly?
YES | - | Go to Step 16 .
NO | - | Replace the reverse lockout solenoid.■
Reinstall the reverse lockout solenoid and reconnect the solenoid 2P connector. Turn the ignition switch ON (II). |